Axiom IoT Batch #04

# Assigment # 06

1. Use led-roulette starter code to blink all the leds in stm32f3 board to run in forward direction.

2. Use led-roulette starter code to blink all the leds in stm32f3 board to run in backward direction.

3.Use led-roulette starter code to blink all the leds in stm32f3 board to run in back and forth ( both backward and forward ) direction at a same time.